{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L8Y1B","FVQ71CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Jäähdytysteho","Nimell.","","kW","","6.8","","12.0","","13.4"]
["Tilan jäähdytys","SEER","","","6.31","6.23","5.61","5.61","5.61"]
["","Vuotuinen energiankulutus","","kWh/a","378","383","593","748.663","749"]
["","Teho","Pdesign","kW","6.80","6.80","9.50","12.00","12.00"]
["","Energiatehokkuusluokka","","","A++","A++","A+","A+","A+"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Teho","Pdesign","kW","6.33","6.33","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","3.87","3.87"]
["","Energiatehokkuusluokka","","","A+","A+","A+","A","A"]
["","Vuotuinen energiankulutus","","kWh/a","2,189","2,189","3,767","4,087.855","4,088"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","","1,010","","1,870","","2,085"]
["","EER","","","","3.37","","3.21","","3.21"]
["","COP","","","","3.64","","3.70","","3.61"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A","","A"]
["","","Lämmitys","","","A","","A"]
["Lämmitysteho","Nimell.","","kW","","7.5","","13.5","","15.5"]
["Huomautukset","","","","","(1) - Vuotuinen energiankulutus ilmoitettu energiamerkintää koskevan direktiivin 2002/31/EY mukaisesti","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","","(2) - SEER ja SCOP ovat EN 14825:n mukaiset","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]