{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXTP-N8"]
[]
[]
[]
[]
["","","","","FVXM25A2V1B / RXTP25N2V1B8","FVXM25A3V1B / RXTP25N2V1B8","FVXM35A2V1B / RXTP35N2V1B8","FVXM35A3V1B / RXTP35N2V1B8"]
["Jäähdytysteho","Min.","","kW","1.40","","1.40"]
["","Maks.","","kW","4.20","","4.30"]
["","Nimell.","","kW","2.50","","3.50"]
["Nimellinen tehokkuus","Annual energy consumption","","kWh","328","","510"]
["","EER","","","3.81","","3.43"]
["","COP","","","3.86","","3.54"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","","A"]
["","","Lämmitys","","A","","B"]
["Lämmitysteho","Nimell.","","kW","3.20","","4.00"]
["","Min.","","kW","1.20","","1.20"]
["","Maks.","","kW","5.70","","6.20"]
["Huomautukset","","","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m.","","(1) - Nimelliset jäähdytystehot perustuvat seuraaviin tietoihin: sisälämpötila: 27°CDB, 19°CWB, ulkolämpötila: 35°CDB, kylmäaineputkiston ekvivalenttipituus: 5 m, korkeusero: 0 m."]
["","","","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m.","","(2) - Nimelliset lämmitystehot perustuvat seuraaviin tietoihin: sisälämpötila: 20°CDB, ulkolämpötila: 7°CDB, 6°CWB, jäähdytysputkisto: 5m, korkeusero: 0 m."]
["","","","","(3) - Katso sähköiset tiedot eri piirustuksista","","(3) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","(4) - Katso toimintalämpötila-alue eri piirustuksesta","","(4) - Katso toimintalämpötila-alue eri piirustuksesta"]
["Jäähdytysteho","Min.","","kW","","1.00","","1.10"]
["","Nimell.","","kW","","2.50","","3.50"]
["","Maks.","","kW","","4.20","","4.30"]
["Lämmitysteho","Min.","","kW","","1.00","","1.10"]
["","Nimell.","","kW","","3.20","","4.00"]
["","Maks.","","kW","","5.70","","6.20"]
["Nimellinen tehokkuus","EER","","","","3.81","","3.43"]
["","COP","","","","3.86","","3.54"]
["","Vuotuinen energiankulutus","","kWh","","328","","510"]
["","Energiamerkintädirektiivi","Jäähdytys","","","A","","A"]
["","","Lämmitys","","","A","","B"]
["Tilan jäähdytys","Energiatehokkuusluokka","","","","A++","","A++"]
["","Teho","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","6.50","","6.10"]
["","Vuotuinen energiankulutus","","kWh/a","","135","","201"]
["Tilojen lämmitys (Keskimääräinen ilmasto)","Energiatehokkuusluokka","","","","A++","","A++"]
["","Teho","Pdesign","kW","","2.50","","3.00"]
["","SCOP/A","","","","4.70","","4.60"]
["","Pdh Lämmitysteho -10°:ssa","","kW","","2.50","","3.00"]
["","Vuotuinen energiankulutus","","kWh/a","","744","","913"]