{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B","FVXM35A3V1B","FVXM50A3V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.02","0.02","0.03"]
["","Lämmitys","","Nimell.","kW","0.02","0.03","0.03"]
["Kotelo","Väri","","","","Valkoinen","Valkoinen","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","600","600","600"]
["","","","Leveys","mm","750","750","750"]
["","","","Syvyys","mm","238","238","238"]
["Paino","Yksikkö","","","kg","17","17","17"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","8.7","9.2","11.6"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7","7","9"]
["","","","Pieni","m³/min","4.9","4.9","6.6"]
["","","","Hiljainen toiminta","m³/min","4.1","4.1","5.4"]
["","","Lämmitys","Suuri","m³/min","9.2","9.8","12.8"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","7.2","7.2","10"]
["","","Lämmitys","Pieni","m³/min","5.6","5.6","8.4"]
["","","","Hiljainen toiminta","m³/min","4.1","4.1","5.9"]
["Äänen tehotaso","Jäähdytys","","","dBA","52","53","61"]
["","Lämmitys","","","dBA","52","53","62"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","38","39","44"]
["","","","Keski","dBA","32","32","38"]
["","","","Pieni","dBA","25","25","31"]
["","","","Hiljainen toiminta","dBA","20","20","27"]
["","Lämmitys","","Suuri","dBA","38","39","46"]
["","","","Keski","dBA","32","32","40"]
["","","","Pieni","dBA","25","25","35"]
["","","","Hiljainen toiminta","dBA","19","19","29"]
["Kylmäaine","GWP","","","","675","675","675"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.4","6.4","6.4"]
["","Kaasu","","Ulkohalkaisija","mm","9.5","9.5","12.7"]
["","Kondenssi","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Langallinen kaukosäädin","","","","BRC073A1","BRC073A1","BRC073A1"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]