{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-M3"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25M3V1B","FVXS35FV1B / RXL35M3V1B"]
["Jäähdytysteho","Nimell.","","kW","2.5","3.5"]
["Nimellinen tehokkuus","Vuotuinen energiankulutus","","kWh","370","535"]
["","EER","","","3.38","3.27"]
["","COP","","","3.78","3.46"]
["","Energiamerkintädirektiivi","Jäähdytys","","A","A"]
["","","Lämmitys","","A","B"]
["Lämmitysteho","Nimell.","","kW","4.5","5.6"]
["Huomautukset","","","","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella","(1) - EER/COP Eurovent 2012 -standardin mukaan, käytettäväksi ainoastaan EU:n ulkopuolella"]
["","","","","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla","(2) - Nimellinen tehokkuus: jäähdytys 35°/27° nimelliskuormalla, lämmitys 7°/20° nimelliskuormalla"]
["","","","","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V"]
["","","","","(6) - Pienintä nimellistä lämmitystehoa varten aseta sisäyksikön puhallin SL-asentoon","(6) - Pienintä nimellistä lämmitystehoa varten aseta sisäyksikön puhallin SL-asentoon"]
["","","","","(7) - Suurin lämmitysteho -15 °C ulkolämpötilassa","(7) - Suurin lämmitysteho -15 °C ulkolämpötilassa"]