{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Vakiovarusteet","Vaatimustenmukaisuusvakuutus","","","","1"]
["Paino","Yksikkö","","","kg","173"]
["Kylmäaine","GWP","","","","1.0"]
["","Täytösmäärä","","","kg","3.20"]
["Puhallinmoottori","Lähtö","","","L","350"]
["Lämmönvaihdin","Tyyppi","","","","Poikkirivoitettu elementti"]
["Mitat","Yksikkö","","Leveys","mm","635"]
["","","","Syvyys","mm","765"]
["","","","Korkeus","mm","1,680"]
["Kotelo","Väri","","","","Norsunluunvalkoinen"]
["Puhallin","Tyyppi","","","","Siipipuhallin"]
["","Ilmamäärä","Jäähdytys","Nimell.","m³/min","102"]
["","Määrä","","","","1"]
["Power supply","Vaihe","","","","3N~"]
["","Taajuus","","","Hz","50"]
["","Jännite","","","V","380-415"]
["Huomautukset","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Kompressori 1"]
["","","","","","(3) - Kompressori 2"]
["","","","","","(4) - Kompressori 3"]
["","","","","","(5) - Tehtaalla tehty lataus"]
["","","","","","(6) - Vain K65 suunnittelupaineella. 120 bar sallittu AC-putkistoliitännöissä."]
["","","","","","(7) - Varoventtiilin paine näytetään mittarin paineena."]
["","","","","","(8) - Vain K65 suunnittelupaineella. 90 bar sallittu kylmäsäilytys-putkistossa."]