{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A8"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B8","RXA25A5V1B8","RXA35A5V1B8"]
["Mitat","Yksikkö","","Korkeus","mm","550","550","550"]
["","","","Leveys","mm","840","840","840"]
["","","","Syvyys","mm","350","350","350"]
["Paino","Yksikkö","","","kg","32","32","32"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46.0","46.0","49.0"]
["","Lämmitys","","Nimell.","dBA","47.0","47.0","49.0"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","0.76","0.76","0.76"]
["","Täytösmäärä","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15.0","15.0","15.0"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Energiatehokkuusalue","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Huomautukset","","","","","(1) - Sisältää fluorattuja kasvihuonekaasuja","(1) - Sisältää fluorattuja kasvihuonekaasuja","(1) - Sisältää fluorattuja kasvihuonekaasuja"]
["","","","","","(2) - Katso toimintalämpötila-alue eri piirustuksesta","(2) - Katso toimintalämpötila-alue eri piirustuksesta","(2) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista","(3) - Katso sähköiset tiedot eri piirustuksista"]
["Vakiovarusteet","Asennusohje","","","","","1","1"]
["","Kylmäaineen määrän tarra","","","","","1","1"]
["","Monikieliset fluorattujen kasvihuonekaasujen merkinnät","","","","","1","1"]
["","Yleiset varotoimet","","","","","1","1"]
["","Tyhjennystulppa","","","","","1","1"]