{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA42B5V1B","RXA50B2V1B","RXA50B5V1B"]
["Mitat","Yksikkö","","Korkeus","mm","734","","734","734"]
["","","","Leveys","mm","870","","870","954"]
["","","","Syvyys","mm","373","","373","401"]
["Paino","Yksikkö","","","kg","50","","50","49"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","","-10","-10"]
["","","","Maks.","°CDB","46","","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","","-15","-15"]
["","","","Maks.","°CWB","18","","18","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","48.0","","48.0","48"]
["","Lämmitys","","Nimell.","dBA","48.0","","48.0","48"]
["Kylmäaine","Tyyppi","","","","R-32","","R-32","R-32"]
["","Täytösmäärä","","","kg","1.10","","1.10","1.1"]
["","Täytösmäärä","","","tCO2Eq","0.75","","0.75","0.75"]
["","GWP","","","","675","","675","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","30","","30","30"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","20","","20","20"]
["Vakiovarusteet","Asennusohje","","","","1","","1","1"]
["","Kylmäaineen määrän tarra","","","","1","","1","1"]
["","Monikieliset fluorattujen kasvihuonekaasujen merkinnät","","","","1","","1","1"]
["","Tyhjennyskorkki","","","","3","","3","3"]
["","Tyhjennystulppa","","","","1","","1","1"]
["Energiatehokkuusalue","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Virransyöttö","Vaihe","","","","1~","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","","50","50"]
["","Jännite","","","V","220-240","","220-240","220-240"]
["Huomautukset","","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","","(1) - Katso toimintalämpötila-alue eri piirustuksesta","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(2) - Katso sähköiset tiedot eri piirustuksista","","(2) - Katso sähköiset tiedot eri piirustuksista","(2) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","(3) - Sisältää fluorattuja kasvihuonekaasuja","","(3) - Sisältää fluorattuja kasvihuonekaasuja","(3) - Sisältää fluorattuja kasvihuonekaasuja"]