{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","30.6","30.6"]
["","","Lämmitys","Erittäin pieni","m³/min","27.2","27.2"]
["","","","Erittäin pieni","cfm","1080","1080"]
["","","Lämmitys","Erittäin pieni","cfm","960","960"]
["Mitat","Yksikkö","","Korkeus","mm","550","550"]
["","","","Leveys","mm","858","858"]
["","","","Syvyys","mm","330","330"]
["Paino","Yksikkö","","","kg","40","40"]
["Kompressori","Type","","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-25","-25"]
["","","","Maks.","°CWB","18","18"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","48","48"]
["","","","Pieni","dBA","44","44"]
["","Lämmitys","","Suuri","dBA","49","49"]
["","","","Pieni","dBA","45","45"]
["Kylmäaine","Tyyppi","","","","R-410A","R-410A"]
["","Täytösmäärä","","","kg","1","1"]
["","Täytösmäärä","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - IU","Maks.","m","15","15"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]