{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["Mitat","Yksikkö","","Korkeus","mm","610"]
["","","","Leveys","mm","923"]
["","","","Syvyys","mm","367"]
["Paino","Yksikkö","","","kg","40"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","600"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (1), 46 (1)"]
["","Lämmitys","Ympäristö","Min.","°CWB","-21 (1), -15 (1)"]
["","","","Maks.","°CWB","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","48"]
["","Lämmitys","","Nimell.","dBA","49"]
["Kylmäaine","Tyyppi","","","","R-32"]
["","Täytösmäärä","","","kg","0.95"]
["","Täytösmäärä","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","30"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","20"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]
["Huomautukset","","","","","(1) - Katso toimintalämpötila-alue eri piirustuksesta"]
["","","","","","(2) - Katso sähköiset tiedot eri piirustuksista"]
["","","","","","(3) - Sisältää fluorattuja kasvihuonekaasuja"]