{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","","48"]
["","Jäähdytys","","Suuri","dBA","","","48"]
["Vakiovarusteet","Asennusohje","","","","","","1"]
["","Kylmäaineen määrän tarra","","","","","","1"]
["","Monikieliset fluorattujen kasvihuonekaasujen merkinnät","","","","","","1"]
["","Tyhjennystulppa (vain lämpöpumppumallit)","","","","","","1"]
["Kylmäaine","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Täytösmäärä","","","kg","","","1.2"]
["","Tyyppi","","","","","","R-410A"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","","","780"]
["","","Lämmitys","Erittäin pieni","r/min","","","740"]
["Operation range","Jäähdytys","Ympäristö","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Heating","Ympäristö","Maks.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Piping connections","Korkeusero","IU - OU","Maks.","m","","","15"]
["","Lisäkylmäainemäärä","","","kg/m","","","0,02 (yli 10m putkistoille)"]
["Mitat","Yksikkö","","Leveys","mm","","","765"]
["","","","Syvyys","mm","","","285"]
["","","","Korkeus","mm","","","550"]
["Kompressori","Type","","","","","","Hermeettisesti suljettu keinukompressori"]
["Paino","Yksikkö","","","kg","","","34"]
["Puhallin","Ilmamäärä","Lämmitys","Erittäin pieni","cfm","","","904"]
["","","","Erittäin pieni","m³/min","","","25.6"]
["","","Jäähdytys","Erittäin pieni","m³/min","","","30.1"]
["","","","Erittäin pieni","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Taajuus","","","Hz","","","50"]
["","Jännite","","","V","","","220-240"]
["Huomautukset","","","","","","","(1) - SL: Ilmanvirtausasetuksen hiljainen asetus puhaltimelle"]
["Puhallin","Ilmamäärä","Jäähdytys","Erittäin pieni","m³/min","30.1","30.1"]
["","","Lämmitys","Erittäin pieni","m³/min","25.6","25.6"]
["","","","Erittäin pieni","cfm","1063","1063"]
["","","Lämmitys","Erittäin pieni","cfm","904","904"]
["Mitat","Yksikkö","","Korkeus","mm","550","550"]
["","","","Leveys","mm","765","765"]
["","","","Syvyys","mm","285","285"]
["Paino","Yksikkö","","","kg","34","34"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","780","780"]
["","","Lämmitys","Erittäin pieni","r/min","740","740"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","46","46"]
["","Lämmitys","","Suuri","dBA","47","47"]
["Kylmäaine","Tyyppi","","","","R-410A","R-410A"]
["","Täytösmäärä","","","kg","1.0","1.0"]
["","Täytösmäärä","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15","15"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]
["Huomautukset","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Vakiovarusteet","Drain plug (only heat pump models)","","","","","1"]