{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-A"]
[]
[]
[]
[]
["","","","","","RXTP25A2V1B","RXTP35A2V1B"]
["Mitat","Yksikkö","","Korkeus","mm","605","605"]
["","","","Leveys","mm","930","930"]
["","","","Syvyys","mm","376","376"]
["Paino","Yksikkö","","","kg","42","42"]
["Puhallinmoottori","Nopeus","Jäähdytys","Erittäin pieni","r/min","800","800"]
["","","Lämmitys","Erittäin pieni","r/min","400","400"]
["Kompressori","Type","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-31","-31"]
["","","","Maks.","°CWB","18","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","48","48"]
["","Lämmitys","","Nimell.","dBA","49.0","49.0"]
["Kylmäaine","Tyyppi","","","","R-32","R-32"]
["","Täytösmäärä","","","kg","0.97","0.97"]
["","Täytösmäärä","","","tCO2Eq","0.66","0.66"]
["","GWP","","","","675.0","675.0"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","20","20"]
["","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 10m putkistoille)","0,02 (yli 10m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15.0","15.0"]
["Vakiovarusteet","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Virransyöttö","Vaihe","","","","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50"]
["","Jännite","","","V","220-240","220-240"]