{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Äänenpaineen taso","Lämmitys","","Nimell.","dBA","","","","52"]
["","Jäähdytys","","Nimell.","dBA","","","","51"]
["Vakiovarusteet","Nippusiteet","","","","","","","2"]
["","Asennusohje","","","","","","","1"]
["","Kylmäaineen merkintä F-kaasun säännös","","","","","","","1"]
["","Yleiset varotoimet","","","","","","","1"]
["","LOT10-energiamerkintä","","","","","","","1"]
["Kylmäaine","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Täytösmäärä","","","kg","","","","3.75"]
["","Tyyppi","","","","","","","R-32"]
["Piping connections","Neste","","Ulkohalkaisija","mm","","","","9.52"]
["","Putkiston pituus","Enint.","OU - IU","m","","","","85"]
["","","Järjestelmä","Täyttämätön","m","","","","40"]
["","","","Ekvivalentti","m","","","","100"]
["","Kaasu","","Ulkohalkaisija","mm","","","","15.9"]
["","Korkeusero","IU - IU","Maks.","m","","","","0.5"]
["","","IU - OU","Maks.","m","","","","30.0"]
["","Lisäkylmäainemäärä","","","kg/m","","","","Katso asennusohje"]
["Äänen tehotaso","Jäähdytys","","","dBA","","","","70"]
["","Lämmitys","","","dBA","","","","70 (1)"]
["Kompressori","Type","","","","","","","Hermeettisesti suljettu keinukompressori"]
["Mitat","Yksikkö","","Leveys","mm","","","","940"]
["","","","Syvyys","mm","","","","320"]
["","","","Korkeus","mm","","","","1,430"]
["Paino","Yksikkö","","","kg","","","","92"]
["Power supply","Phase","","","","","","","1~"]
["","Taajuus","","","Hz","","","","50"]
["","Jännite","","","V","","","","220-240"]
["Huomautukset","","","","","","","","(1) - ENER Lot 21 mukaisesti"]
["","","","","","","","","(2) - Eurooppalainen/kansainvälinen tekninen standardi, jossa määritellään rajat harmoniselle virralle, jonka tuottavat julkiseen matalan jännitteen järjestelmään kytketyt laitteet, joiden syöttövirta on suurempi kuin 16 A ja ≤ 75 A vaihetta kohti."]
["","","","","","","","","(3) - Ssc: oikosulkuteho"]
["","","","","","","","","(4) - Eurooppalainen/kansainvälinen tekninen standardi, jossa määritellään rajat harmoniselle virralle, jonka tuottavat julkiseen matalan jännitteen järjestelmään kytketyt laitteet, joiden syöttövirta ≤ 16A vaihetta kohti."]
["Mitat","Yksikkö","","Korkeus","mm","990","1430","1430"]
["","","","Leveys","mm","940","940","940"]
["","","","Syvyys","mm","320","320","320"]
["Paino","Yksikkö","","","kg","70","92","92"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-20","-20","-20"]
["","","","Maks.","°CDB","52","52","52"]
["","Lämmitys","Ympäristö","Min.","°CWB","-20","-20","-20"]
["","","","Maks.","°CWB","18.0","18.0","18.0"]
["Äänen tehotaso","Jäähdytys","","","dBA","64","66","69"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","46","47","50"]
["","Lämmitys","","Nimell.","dBA","49","51","52"]
["Kylmäaine","Tyyppi","","","","R-32","R-32","R-32"]
["","Täytösmäärä","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Täytösmäärä","","","tCO2Eq","1.99","2.53","2.53"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","9.52","9.52","9.52"]
["","Kaasu","","Ulkohalkaisija","mm","15.9","15.9","15.9"]
["Putkistoliitännät","Putkiston pituus","Enint.","OU - IU","m","55","85","85"]
["","","Järjestelmä","Ekvivalentti","m","75","100","100"]
["","","","Täyttämätön","m","40","40","40"]
["","Lisäkylmäainemäärä","","","kg/m","Katso asennusohje","Katso asennusohje","Katso asennusohje"]
["","Korkeusero","IU - OU","Maks.","m","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5"]
["Vakiovarusteet","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Virransyöttö","Vaihe","","","","1~","1~","1~"]
["Syöttöjännite","Taajuus","","","Hz","50","50","50"]
["","Jännite","","","V","220-240","220-240","220-240"]
["Virta - 50&nbsp;Hz","Virta - 50&nbsp;Hz-=-Sulakkeiden enimmäisvirta (MFA)-=-A","","","A","20","32","32"]
["Äänen tehotaso","Lämmitys","","","dBA","","","69 (1)"]
["Huomautukset","","","","","","","(1) - ENER Lot 21 mukaisesti"]