{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Sovellus","","","","","Lattialle asennettava"]
["Teho","m³/min","","","","33.33"]
["Kotelo","Väri","","","","Maalattu galvanoitu teräslevy"]
["Mitat","Yksikkö","","Korkeus","mm","1628"]
["","","","Leveys","mm","720"]
["","","","Syvyys","mm","770"]
["Paino","Yksikkö","","","kg","150"]
["Soveltuva huonekoko","m²","","","","133"]
["Ilmanpuhdistustoiminto","Ottoteho","","H","kW","0.379"]
["Äänenpaineen taso","Ilmanpuhdistustoiminto","","Suuri","dBA","55.9"]
["Puhallin","Ilmamäärä","Ilmanpuhdistustoiminto","Turbo","m³/h","2300"]
["","","","Suuri","m³/h","2000"]
["Turvalaitteet","Kohde","","01","","Turvakytkin (toiminta pysähtyy, kun takaluukku avautuu)"]
["Vakiovarusteet","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Virtajohto","m","","","","3"]
["Syöttöjännite","Taajuus","","","Hz","50/60"]
["Virta käynnissä","Ilmanpuhdistustoiminto","","Suuri","A","1.73"]